TeamTalk 5 Java DLL Version 5.19A

Static Public Attributes | List of all members
BearWare.SoundDeviceConstants Struct Reference
Sound Capture and Playback

IDs for sound devices. More...

## Static Public Attributes

const int | TT_SOUNDDEVICE_ID_REMOTEIO = 0
| Sound device ID for iOS AudioUnit subtype Remote I/O Unit. More...
const int | TT_SOUNDDEVICE_ID_VOICEPREPROCESSINGIO = (1 | (int)TT_SOUNDDEVICE_ID_SHARED_FLAG)
| Sound device ID for iOS AudioUnit subtype Voice-Processing I/O Unit. This sound device ID include the flag BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_SHARED_FLAG since multiple streams cannot be recorded/played on the device. More...
const int | TT_SOUNDDEVICE_ID_OPENSLES_DEFAULT = 0
| Sound device ID for Android OpenSL ES default audio device. Note that this sound device may also exist in the form where the `nDeviceID` as been or'ed with BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_SHARED_FLAG. More...
const int | TT_SOUNDDEVICE_ID_OPENSLES_VOICECOM = 1
| Sound device ID for Android OpenSL ES voice communication mode. This device uses the OpenSL ES' AndroidConfiguration `SL_ANDROID_RECORDING_PRESET_VOICE_COMMUNICATION`. More...
const int | TT_SOUNDDEVICE_ID_TEAMTALK_VIRTUAL = 1978
| Sound device ID for virtual TeamTalk sound device. More...
const uint | TT_SOUNDDEVICE_ID_SHARED_FLAG = 0x00000800
| Flag/bit in `nDeviceID` telling if the BearWare.SoundDevice is a shared version of an existing sound device. More...
const uint | TT_SOUNDDEVICE_ID_MASK = 0x000007FF
| Extract sound device ID of `nDeviceID` in BearWare.SoundDevice by and'ing this value. More...

## Detailed Description

IDs for sound devices.

Definition at line 336 of file TeamTalk.cs.

## Member Data Documentation

## ◆ TT_SOUNDDEVICE_ID_REMOTEIO

const int BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_REMOTEIO = 0

static

Sound device ID for iOS AudioUnit subtype Remote I/O Unit.

See also
  SOUNDSYSTEM_AUDIOUNIT

Definition at line 340 of file TeamTalk.cs.

## ◆ TT_SOUNDDEVICE_ID_VOICEPREPROCESSINGIO

const int BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_VOICEPREPROCESSINGIO = (1 | (int)TT_SOUNDDEVICE_ID_SHARED_FLAG)

static

Sound device ID for iOS AudioUnit subtype Voice-Processing I/O Unit. This sound device ID include the flag BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_SHARED_FLAG since multiple streams cannot be recorded/played on the device.

See also
  SoundSystem.SOUNDSYSTEM_AUDIOUNIT

Definition at line 346 of file TeamTalk.cs.

## ◆ TT_SOUNDDEVICE_ID_OPENSLES_DEFAULT

const int BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_OPENSLES_DEFAULT = 0

static

Sound device ID for Android OpenSL ES default audio device. Note that this sound device may also exist in the form where the `nDeviceID` as been or'ed with BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_SHARED_FLAG.

See also
  SOUNDSYSTEM_OPENSLES_ANDROID

Definition at line 351 of file TeamTalk.cs.

## ◆ TT_SOUNDDEVICE_ID_OPENSLES_VOICECOM

const int BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_OPENSLES_VOICECOM = 1

static

Sound device ID for Android OpenSL ES voice communication mode. This device uses the OpenSL ES' AndroidConfiguration `SL_ANDROID_RECORDING_PRESET_VOICE_COMMUNICATION`.

See also
  SoundSystem.SOUNDSYSTEM_OPENSLES_ANDROID

Definition at line 356 of file TeamTalk.cs.

## ◆ TT_SOUNDDEVICE_ID_TEAMTALK_VIRTUAL

const int BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_TEAMTALK_VIRTUAL = 1978

static

Sound device ID for virtual TeamTalk sound device.

This is a sound device which decodes received audio packets but does not send the decoded audio to a real sound device. When used for recording the virtual sound device injects silence.

In duplex mode the virtual TeamTalk sound device can only be used as input/output device.

See also
  SOUNDSYSTEM_NONE

Definition at line 365 of file TeamTalk.cs.

## ◆ TT_SOUNDDEVICE_ID_SHARED_FLAG

const uint BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_SHARED_FLAG = 0x00000800

static

Flag/bit in `nDeviceID` telling if the BearWare.SoundDevice is a shared version of an existing sound device.

On Android the recording device can only be used by one TeamTalk instance. As a workaround for this issue a shared recording device has been introduced. Internally TeamTalk initializes BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_OPENSLES_DEFAULT which then resample and distribution the audio data to multiple TeamTalk instances.

The shared audio device on Android will show up as (TT_SOUNDDEVICE_ID_OPENSLES_DEFAULT | TT_SOUNDDEVICE_ID_SHARED_FLAG), i.e. 2048.

Definition at line 381 of file TeamTalk.cs.

## ◆ TT_SOUNDDEVICE_ID_MASK

const uint BearWare.SoundDeviceConstants.TT_SOUNDDEVICE_ID_MASK = 0x000007FF

static

Extract sound device ID of `nDeviceID` in BearWare.SoundDevice by and'ing this value.

let PhysicalDeviceID = (SoundDevice.nDeviceID & TT_SOUNDDEVICE_ID_MASK).

Definition at line 387 of file TeamTalk.cs.