TeamTalk 5 Java DLL Version 5.22A

Loading...
Searching...
No Matches
Public Attributes | List of all members
BearWare.OpusCodec Struct Reference
Audio and Video Codecs

OPUS audio codec settings. For detailed information about the OPUS codec check out http://www.opus-codec.org. More...

## Public Attributes

int | nSampleRate
| The sample rate to use. Sample rate must be 8000, 12000, 16000, 24000 or 48000 Hz.
int | nChannels
| Mono = 1 or stereo = 2.
int | nApplication
| Application of encoded audio, VoIP or music.
int | nComplexity
| Complexity of encoding (affects CPU usage). Value from 0-10.
bool | bFEC
| Forward error correction. Corrects errors if there's packetloss.
bool | bDTX
| Discontinuous transmission. Enables "null" packets during silence.
int | nBitRate
| Bitrate for encoded audio. Should be between BearWare.OpusConstants.OPUS_MIN_BITRATE and BearWare.OpusConstants.OPUS_MAX_BITRATE.
bool | bVBR
| Enable variable bitrate.
bool | bVBRConstraint
| Enable constrained VBR. `bVBR` must be enabled to enable this.
int | nTxIntervalMSec
| Duration of audio before each transmission. Minimum is 2 msec. Recommended is 40 msec. Maximum is 500 msec.
int | nFrameSizeMSec
| OPUS supports 2.5, 5, 10, 20, 40, 60, 80, 100 and 120 msec. If `nFrameSizeMSec` is 0 then `nFrameSizeMSec` will be same as `nTxIntervalMSec`.

## Detailed Description

OPUS audio codec settings. For detailed information about the OPUS codec check out http://www.opus-codec.org.

Definition at line 1048 of file TeamTalk.cs.

## Member Data Documentation

## ◆ nSampleRate

int BearWare.OpusCodec.nSampleRate

The sample rate to use. Sample rate must be 8000, 12000, 16000, 24000 or 48000 Hz.

Definition at line 1052 of file TeamTalk.cs.

## ◆ nChannels

int BearWare.OpusCodec.nChannels

Mono = 1 or stereo = 2.

Definition at line 1054 of file TeamTalk.cs.

## ◆ nApplication

int BearWare.OpusCodec.nApplication

Application of encoded audio, VoIP or music.

See also
  OPUS_APPLICATION_VOIP
  OPUS_APPLICATION_AUDIO

Definition at line 1058 of file TeamTalk.cs.

## ◆ nComplexity

int BearWare.OpusCodec.nComplexity

Complexity of encoding (affects CPU usage). Value from 0-10.

Definition at line 1061 of file TeamTalk.cs.

## ◆ bFEC

bool BearWare.OpusCodec.bFEC

Forward error correction. Corrects errors if there's packetloss.

Definition at line 1064 of file TeamTalk.cs.

## ◆ bDTX

bool BearWare.OpusCodec.bDTX

Discontinuous transmission. Enables "null" packets during silence.

Definition at line 1067 of file TeamTalk.cs.

## ◆ nBitRate

int BearWare.OpusCodec.nBitRate

Bitrate for encoded audio. Should be between BearWare.OpusConstants.OPUS_MIN_BITRATE and BearWare.OpusConstants.OPUS_MAX_BITRATE.

Definition at line 1071 of file TeamTalk.cs.

## ◆ bVBR

bool BearWare.OpusCodec.bVBR

Enable variable bitrate.

Definition at line 1073 of file TeamTalk.cs.

## ◆ bVBRConstraint

bool BearWare.OpusCodec.bVBRConstraint

Enable constrained VBR. `bVBR` must be enabled to enable this.

Definition at line 1076 of file TeamTalk.cs.

## ◆ nTxIntervalMSec

int BearWare.OpusCodec.nTxIntervalMSec

Duration of audio before each transmission. Minimum is 2 msec. Recommended is 40 msec. Maximum is 500 msec.

The BearWare.SoundSystem must be able to process audio packets at this interval. In most cases this makes less than 40 msec transmission interval unfeasible.

Definition at line 1083 of file TeamTalk.cs.

## ◆ nFrameSizeMSec

int BearWare.OpusCodec.nFrameSizeMSec

OPUS supports 2.5, 5, 10, 20, 40, 60, 80, 100 and 120 msec. If `nFrameSizeMSec` is 0 then `nFrameSizeMSec` will be same as `nTxIntervalMSec`.

Definition at line 1087 of file TeamTalk.cs.